Project: Kiosk-Landscaping

Description: Build up to 2 levels of landscaping

timbers, 1 foot apart to slow the soil

undermining and add support to the

foundation. Add drain pipe with holes

for drainage. Fill with dirt and rock.

Materials: 21-8’ landscape timbers

Nails(large to connect timbers), 3-

Large bags of concrete, stakes, string,

Corrugated pipe about 40’ with holes

Rock and soil.

Tools: chain saw, 4+ hammers, level, line level

Pick, 3 shovels, post hole digger, square,

Wheel barrow, hose.

People: 8-4 hours: 32 hours total