Project: Kiosk-Landscaping

Description: Build up to 2 levels of landscaping

 timbers, 1 foot apart to slow the soil

 undermining and add support to the

 foundation. Add drain pipe with holes

 for drainage. Fill with dirt and rock.

Materials: 21-8’ landscape timbers

 Nails(large to connect timbers), 3-

 Large bags of concrete, stakes, string,

 Corrugated pipe about 40’ with holes

 Rock and soil.

Tools: chain saw, 4+ hammers, level, line level

 Pick, 3 shovels, post hole digger, square,

 Wheel barrow, hose.

People: 8-4 hours: 32 hours total