|  |  |  |
| --- | --- | --- |
| Pelican-Case.com - You break it, we replace it... forever. |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|

|  |
| --- |
|  |

C:\Users\Carole's Dell\Desktop\Pelican cooler.jpg | **Pelican ProGear™ Elite Cooler - 45 Quart**

|  |  |
| --- | --- |
|  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

* [**Description**](http://www.pelican-case.com/45q-white.html#tab1)

**Pelican ProGear™ Elite Cooler/Ice Chest Series - 45 quart** *PACK A TOUGHER, COLDER COOLER ON YOUR NEXT BIG WATER ADVENTURE.* Introducing ProGear™ Coolers from Pelican Products ProGear™ Line. These coolers boast best in class ice retention and Pelican's unconditional lifetime guarantee. *View the Pelican ProGear Maximum Ice Retention Video* **Features:**   Best in class ice retention.   Injection Molded Swing handles with overmolded grip   UV Protected Shell   Durable Rotomolded Shell   Made in the USA   Unconditional Lifetime Guarantee   Fish measuring ruler molded on lid   Threaded leak proof recessed drain plug   Easy open locking latches **45Q-MC-WHT ProGear™ Cooler 45Qt**Cooler Internal Dimensions 19.00”L x 12.00”W x 12.00” DOverall Exterior Dimensions 29.66”L x 20.00”W x 19.25”DWeight 35.80 lbs.Cooler Internal Volume 49.50 QuartsCooler Material PolyethyleneHandle / Latch Material / Spigot TPE / ABS / PPHardware Stainless SteelInsulation Polyurethane 2” thickness

|  |  |
| --- | --- |
|  |  |

|  |
| --- |
|  |
|  |  |  |

 |  |