|  |  |  |
| --- | --- | --- |
| [Pelican-Case.com - You break it, we replace it... forever.](http://www.pelican-case.com/index.html) |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | |  |  |
| |  | | --- | |  |   C:\Users\Carole's Dell\Desktop\Pelican cooler.jpg | | **Pelican ProGear™ Elite Cooler - 45 Quart**   |  |  | | --- | --- | |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | |  |  |  |  |  | |  |  |  |  |  |      * [**Description**](http://www.pelican-case.com/45q-white.html#tab1)   **Pelican ProGear™ Elite Cooler/Ice Chest Series - 45 quart**   *PACK A TOUGHER, COLDER COOLER ON YOUR NEXT BIG WATER ADVENTURE.*   Introducing ProGear™ Coolers from Pelican Products ProGear™ Line. These coolers boast best in class ice retention and Pelican's unconditional lifetime guarantee.   *View the Pelican ProGear Maximum Ice Retention Video*    **Features:**    Best in class ice retention.    Injection Molded Swing handles with overmolded grip    UV Protected Shell    Durable Rotomolded Shell    Made in the USA    Unconditional Lifetime Guarantee    Fish measuring ruler molded on lid    Threaded leak proof recessed drain plug    Easy open locking latches   **45Q-MC-WHT ProGear™ Cooler 45Qt** Cooler Internal Dimensions 19.00”L x 12.00”W x 12.00” D Overall Exterior Dimensions 29.66”L x 20.00”W x 19.25”D Weight 35.80 lbs. Cooler Internal Volume 49.50 Quarts Cooler Material Polyethylene Handle / Latch Material / Spigot TPE / ABS / PP Hardware Stainless Steel Insulation Polyurethane 2” thickness   |  |  | | --- | --- | |  |  |  |  |  |  | | --- | --- | --- | |  | | | |  |  |  | |  | |